IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "// PROJECT/NUMBER //"
Time stamp: "2020-11-27T09:24:01"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.10.26 - Exporter 21.1.10.26 - Alternate UI 21.1.10.26"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "//" "AUTHOR" "//" of Organization "// ORGANIZATION/NAME //" description "// ORGANIZATION/DESCRIPTION //"
  Owner history of Person "//" "AUTHOR" "//" of Organization "// ORGANIZATION/NAME //" description "// ORGANIZATION/DESCRIPTION //" | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1606464608 (2020-11-27T08:10:08Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "// PROJECT/NUMBER //" | long name "// PROJECT/NAME //" | phase "// PROJECT/STATUS //"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING "// BUILDING/NAME //" | long name "// BUILDING/NAME //" | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 18 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Outside wall" | object type "Basic Wall:Outside wall" | names: "Basic Wall:Outside wall:358471", "Basic Wall:Outside wall:358528", "Basic Wall:Outside wall:358604" (+1 more) | material: layers "Basic Wall:Outside wall" ("Default Wall" 200.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "M_Door-Interior-Double-Full Glass-Wood:1500 x 2000mm" | object type "M_Door-Interior-Double-Full Glass-Wood:1500 x 2000mm" | names: "M_Door-Interior-Double-Full Glass-Wood:1500 x 2000mm:358703" | material: materials ("Aluminum", "Cherry", "Glass") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Custom_Pset
          2 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:Outside door" | object type "M_Single-Flush:Outside door" | names: "M_Single-Flush:Outside door:358883", "M_Single-Flush:Outside door:359319" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Custom_Pset
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Inside" | object type "Basic Wall:Inside" | names: "Basic Wall:Inside:359210", "Basic Wall:Inside:359304" | material: layers "Basic Wall:Inside" ("Default Wall" 200.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:Inside Door" | object type "M_Single-Flush:Inside Door" | names: "M_Single-Flush:Inside Door:359375" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Custom_Pset
          1 x IFCDOOR | type IFCDOORSTYLE "M_Single-Flush:Inside Door" | object type "M_Single-Flush:Inside Door" | names: "M_Single-Flush:Inside Door:359428" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_ConcreteElementGeneral, Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Custom_Pset
          6 x IFCWINDOW | type IFCWINDOWSTYLE "M_Fixed:0915 x 1830mm" | object type "M_Fixed:0915 x 1830mm" | names: "M_Fixed:0915 x 1830mm:359493", "M_Fixed:0915 x 1830mm:359637", "M_Fixed:0915 x 1830mm:359681" (+3 more) | material: materials ("Glass", "Sash") | property sets: Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Custom_Pset, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 150mm" | object type "Floor:Generic 150mm" | FLOOR | names: "Floor:Generic 150mm:360649" | material: layers "Floor:Generic 150mm" ("Default Floor" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Custom_Pset
        IFCSPACE "10" | long name "Room" | INTERNAL
        IFCSPACE "11" | long name "Room" | INTERNAL
        IFCSPACE "12" | long name "Room" | INTERNAL
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | object type "Level:8mm Head" | elevation 4000.
        contains 14 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Outside wall" | object type "Basic Wall:Outside wall" | names: "Basic Wall:Outside wall:358471", "Basic Wall:Outside wall:358528", "Basic Wall:Outside wall:358604" (+1 more) | material: layers "Basic Wall:Outside wall" ("Default Wall" 200.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Inside" | object type "Basic Wall:Inside" | names: "Basic Wall:Inside:359210", "Basic Wall:Inside:359304" | material: layers "Basic Wall:Inside" ("Default Wall" 200.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 150mm" | object type "Floor:Generic 150mm" | FLOOR | names: "Floor:Generic 150mm:360659" | material: layers "Floor:Generic 150mm" ("Default Floor" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Custom_Pset
          7 x IFCWINDOW | type IFCWINDOWSTYLE "M_Fixed:0915 x 1830mm" | object type "M_Fixed:0915 x 1830mm" | names: "M_Fixed:0915 x 1830mm:360741", "M_Fixed:0915 x 1830mm:360742", "M_Fixed:0915 x 1830mm:360743" (+4 more) | material: materials ("Glass", "Sash") | property sets: Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Custom_Pset, BaseQuantities
      IFCBUILDINGSTOREY "Level 4" | long name "Level 4" | object type "Level:8mm Head" | elevation 8000.
        contains 11 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Outside wall" | object type "Basic Wall:Outside wall" | names: "Basic Wall:Outside wall:358471", "Basic Wall:Outside wall:358528", "Basic Wall:Outside wall:358604" (+1 more) | material: layers "Basic Wall:Outside wall" ("Default Wall" 200.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Inside" | object type "Basic Wall:Inside" | names: "Basic Wall:Inside:359210", "Basic Wall:Inside:359304" | material: layers "Basic Wall:Inside" ("Default Wall" 200.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 150mm" | object type "Floor:Generic 150mm" | FLOOR | names: "Floor:Generic 150mm:360669" | material: layers "Floor:Generic 150mm" ("Default Floor" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Custom_Pset
          4 x IFCWINDOW | type IFCWINDOWSTYLE "M_Fixed:0915 x 1830mm" | object type "M_Fixed:0915 x 1830mm" | names: "M_Fixed:0915 x 1830mm:361212", "M_Fixed:0915 x 1830mm:361328", "M_Fixed:0915 x 1830mm:361430" (+1 more) | material: materials ("Glass", "Sash") | property sets: Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Custom_Pset, BaseQuantities
      IFCBUILDINGSTOREY "Level 5" | long name "Level 5" | object type "Level:8mm Head" | elevation 12000.
        contains 11 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Outside wall" | object type "Basic Wall:Outside wall" | names: "Basic Wall:Outside wall:358471", "Basic Wall:Outside wall:358528", "Basic Wall:Outside wall:358604" (+1 more) | material: layers "Basic Wall:Outside wall" ("Default Wall" 200.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Inside" | object type "Basic Wall:Inside" | names: "Basic Wall:Inside:359210", "Basic Wall:Inside:359304" | material: layers "Basic Wall:Inside" ("Default Wall" 200.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 150mm" | object type "Floor:Generic 150mm" | FLOOR | names: "Floor:Generic 150mm:360679" | material: layers "Floor:Generic 150mm" ("Default Floor" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Custom_Pset
          4 x IFCWINDOW | type IFCWINDOWSTYLE "M_Fixed:0915 x 1830mm" | object type "M_Fixed:0915 x 1830mm" | names: "M_Fixed:0915 x 1830mm:361674", "M_Fixed:0915 x 1830mm:361738", "M_Fixed:0915 x 1830mm:361840" (+1 more) | material: materials ("Glass", "Sash") | property sets: Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon, Custom_Pset, BaseQuantities
      IFCBUILDINGSTOREY "Level 6" | long name "Level 6" | object type "Level:8mm Head" | elevation 16000.
        contains 1 element
          1 x IFCROOF | object type "Basic Roof:Generic - 400mm" | names: "Basic Roof:Generic - 400mm:360689" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Custom_Pset, Constraints

Types
  IFCWALLTYPE "Basic Wall:Outside wall" | STANDARD | 16 occurrences | material: layers "Basic Wall:Outside wall" ("Default Wall" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ConcreteElementGeneral
  IFCDOORSTYLE "M_Door-Interior-Double-Full Glass-Wood:1500 x 2000mm" | DOUBLE_DOOR_SINGLE_SWING_OPPOSITE_LEFT | 1 occurrence | material: materials ("Cherry", "Aluminum", "Cherry", "Cherry") | property sets: M_Door-Interior-Double-Full Glass-Wood:1500 x 2000mm:358703, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "M_Single-Flush:Outside door" | SINGLE_SWING_RIGHT | 2 occurrences | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Single-Flush:Outside door:358883, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:Inside" | STANDARD | 8 occurrences | material: layers "Basic Wall:Inside" ("Default Wall" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ConcreteElementGeneral
  IFCDOORSTYLE "M_Single-Flush:Inside Door" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Panel", "Door - Frame") | property sets: M_Single-Flush:Inside Door:359375, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "M_Single-Flush:Inside Door" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "M_Fixed:0915 x 1830mm" | 21 occurrences | material: materials ("Sash", "Sash", "Sash", "Glass") | property sets: M_Fixed:0915 x 1830mm:359493, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCSLABTYPE "Floor:Generic 150mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic 150mm" ("Default Floor" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCSLABTYPE "Floor:Generic 150mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic 150mm" ("Default Floor" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCSLABTYPE "Floor:Generic 150mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic 150mm" ("Default Floor" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading
  IFCSLABTYPE "Floor:Generic 150mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic 150mm" ("Default Floor" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other, Pset_ElementShading

Property sets
  Pset_ProductRequirements | properties | on 24 objects (24 IFCWALLSTANDARDCASE) | on 2 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 21 objects (21 IFCWINDOW) | on 1 type object
    Category = "Windows" (IFCLABEL)
  Pset_ProductRequirements | properties | on 5 objects (5 IFCDOOR) | on 4 type objects
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 4 objects (4 IFCSLAB) | on 4 type objects
    Category = "Floors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 3 objects (3 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Name = "Room" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Category = "Roofs" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements: 4 more contents on 4 objects not shown
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "// AUTHOR //" (IFCTEXT)
    Building Name = "// BUILDING/NAME //" (IFCTEXT)
    Organization Description = "// ORGANIZATION/DESCRIPTION //" (IFCTEXT)
    Organization Name = "// ORGANIZATION/NAME //" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCWINDOW)
    Mark = "43" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCWINDOW)
    Mark = "44" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCWINDOW)
    Mark = "45" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCWINDOW)
    Mark = "46" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCSPACE)
    Name = "Room" (IFCTEXT)
    Number = "10" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCSPACE)
    Name = "Room" (IFCTEXT)
    Number = "11" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCSPACE)
    Name = "Room" (IFCTEXT)
    Number = "12" (IFCTEXT)
  Identity Data: 30 more contents on 23 objects not shown
  Other | properties | on 21 objects (21 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
    Family = "M_Fixed: 0915 x 1830mm" (IFCLABEL)
    Family and Type = "M_Fixed: 0915 x 1830mm" (IFCLABEL)
    Head Height = 2135. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: Outside wall" (IFCLABEL)
    Type = "M_Fixed: 0915 x 1830mm" (IFCLABEL)
    Type Id = "M_Fixed: 0915 x 1830mm" (IFCLABEL)
  Other | properties | on 16 objects (16 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: Outside wall" (IFCLABEL)
    Family and Type = "Basic Wall: Outside wall" (IFCLABEL)
    Type = "Basic Wall: Outside wall" (IFCLABEL)
    Type Id = "Basic Wall: Outside wall" (IFCLABEL)
  Other | properties | on 8 objects (8 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: Inside" (IFCLABEL)
    Family and Type = "Basic Wall: Inside" (IFCLABEL)
    Type = "Basic Wall: Inside" (IFCLABEL)
    Type Id = "Basic Wall: Inside" (IFCLABEL)
  Other | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 4 objects (4 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: Generic 150mm" (IFCLABEL)
    Family and Type = "Floor: Generic 150mm" (IFCLABEL)
    Type = "Floor: Generic 150mm" (IFCLABEL)
    Type Id = "Floor: Generic 150mm" (IFCLABEL)
  Other | properties | on 3 objects (3 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Phase Id = "New Construction" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "// CLIENT/NAME //" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "// ISSUE DATE //" (IFCTEXT)
    Project Name = "// PROJECT/NAME //" (IFCTEXT)
    Project Number = "// PROJECT/NUMBER //" (IFCTEXT)
    Project Status = "// PROJECT/STATUS //" (IFCTEXT)
  Other | properties | on 2 objects (2 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "M_Single-Flush: Outside door" (IFCLABEL)
    Family and Type = "M_Single-Flush: Outside door" (IFCLABEL)
    Head Height = 2134. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: Outside wall" (IFCLABEL)
    Type = "M_Single-Flush: Outside door" (IFCLABEL)
    Type Id = "M_Single-Flush: Outside door" (IFCLABEL)
  Other: 8 more contents on 4 objects not shown
  Pset_AirSideSystemInformation | properties | on 3 objects (3 IFCSPACE)
    Name = "Room" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 2" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 4" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 5" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 6" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Reference = "Room 10" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Reference = "Room 11" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Reference = "Room 12" (IFCIDENTIFIER)
  Custom_Pset | properties | on 7 objects (7 IFCWINDOW)
    Height = 1830. (IFCLENGTHMEASURE) [MILLI METRE]
    Hyperlink = "Window: URL" (IFCTEXT)
    Keynote = "Window: Keynote" (IFCLABEL)
    NetArea = 3.17875400000013 (IFCAREAMEASURE) [SQUARE_METRE]
    SillHeight = 305.000000000004 (IFCLENGTHMEASURE) [MILLI METRE]
    StatusConstruction = "New Construction" (IFCLABEL)
    StoreyName = "Level: Level 2" (IFCTEXT)
    TypeDescription = "Window: Description" (IFCTEXT)
    TypeMark = "Window: Type Mark" (IFCLABEL)
    Width = 915. (IFCLENGTHMEASURE) [MILLI METRE]
  Custom_Pset | properties | on 6 objects (6 IFCWINDOW)
    Height = 1830. (IFCLENGTHMEASURE) [MILLI METRE]
    Hyperlink = "Window: URL" (IFCTEXT)
    Keynote = "Window: Keynote" (IFCLABEL)
    NetArea = 3.17875400000013 (IFCAREAMEASURE) [SQUARE_METRE]
    SillHeight = 305.000000000004 (IFCLENGTHMEASURE) [MILLI METRE]
    StatusConstruction = "New Construction" (IFCLABEL)
    StoreyName = "Level: Level 1" (IFCTEXT)
    TypeDescription = "Window: Description" (IFCTEXT)
    TypeMark = "Window: Type Mark" (IFCLABEL)
    Width = 915. (IFCLENGTHMEASURE) [MILLI METRE]
  Custom_Pset | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Height = 16000. (IFCLENGTHMEASURE) [MILLI METRE]
    Hyperlink = "_URL_" (IFCTEXT)
    Keynote = "_KEYNOTE_" (IFCLABEL)
    Length = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
    NetArea = 116.574400000001 (IFCAREAMEASURE) [SQUARE_METRE]
    StatusConstruction = "New Construction" (IFCLABEL)
    StoreyName = "Level: Level 1" (IFCTEXT)
    TypeDescription = "_DESCRIPTION_" (IFCTEXT)
    TypeMark = "_TYPE-MARK_" (IFCLABEL)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
  Custom_Pset | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Height = 16000. (IFCLENGTHMEASURE) [MILLI METRE]
    Hyperlink = "_URL_" (IFCTEXT)
    Keynote = "_KEYNOTE_" (IFCLABEL)
    Length = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
    NetArea = 122.89478 (IFCAREAMEASURE) [SQUARE_METRE]
    StatusConstruction = "New Construction" (IFCLABEL)
    StoreyName = "Level: Level 1" (IFCTEXT)
    TypeDescription = "_DESCRIPTION_" (IFCTEXT)
    TypeMark = "_TYPE-MARK_" (IFCLABEL)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
  Custom_Pset | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Height = 16000. (IFCLENGTHMEASURE) [MILLI METRE]
    Hyperlink = "_URL_" (IFCTEXT)
    Keynote = "_KEYNOTE_" (IFCLABEL)
    Length = 8000.00000000004 (IFCLENGTHMEASURE) [MILLI METRE]
    NetArea = 113.404400000001 (IFCAREAMEASURE) [SQUARE_METRE]
    StatusConstruction = "New Construction" (IFCLABEL)
    StoreyName = "Level: Level 1" (IFCTEXT)
    TypeDescription = "_DESCRIPTION_" (IFCTEXT)
    TypeMark = "_TYPE-MARK_" (IFCLABEL)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
  Custom_Pset | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Height = 16000. (IFCLENGTHMEASURE) [MILLI METRE]
    Hyperlink = "_URL_" (IFCTEXT)
    Keynote = "_KEYNOTE_" (IFCLABEL)
    Length = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
    NetArea = 112.119 (IFCAREAMEASURE) [SQUARE_METRE]
    StatusConstruction = "New Construction" (IFCLABEL)
    StoreyName = "Level: Level 1" (IFCTEXT)
    TypeDescription = "_DESCRIPTION_" (IFCTEXT)
    TypeMark = "_TYPE-MARK_" (IFCLABEL)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
  Custom_Pset | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Height = 16000. (IFCLENGTHMEASURE) [MILLI METRE]
    Hyperlink = "_URL_" (IFCTEXT)
    Keynote = "_KEYNOTE_" (IFCLABEL)
    Length = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
    NetArea = 120.89478 (IFCAREAMEASURE) [SQUARE_METRE]
    StatusConstruction = "New Construction" (IFCLABEL)
    StoreyName = "Level: Level 1" (IFCTEXT)
    TypeDescription = "_DESCRIPTION_" (IFCTEXT)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
  Custom_Pset | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Height = 16000. (IFCLENGTHMEASURE) [MILLI METRE]
    Hyperlink = "_URL_" (IFCTEXT)
    Keynote = "_KEYNOTE_" (IFCLABEL)
    Length = 4000.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    NetArea = 60.8000000000001 (IFCAREAMEASURE) [SQUARE_METRE]
    StatusConstruction = "New Construction" (IFCLABEL)
    StoreyName = "Level: Level 1" (IFCTEXT)
    TypeDescription = "_DESCRIPTION_" (IFCTEXT)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
  Custom_Pset: 24 more contents on 27 objects not shown
  BaseQuantities | quantities | on 21 objects (21 IFCWINDOW)
    Area = 3.17875400000013 [SQUARE_METRE]
    Height = 1830. [MILLI METRE]
    Width = 915. [MILLI METRE]
  BaseQuantities | quantities | on 20 objects (20 IFCOPENINGELEMENT)
    Depth = 200. [MILLI METRE]
    Height = 914.999999999999 [MILLI METRE]
    Width = 1830. [MILLI METRE]
  BaseQuantities | quantities | on 5 objects (5 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 1.56 [SQUARE_METRE]
    Height = 4000. [MILLI METRE]
    Length = 7800. [MILLI METRE]
    NetSideArea = 31200000. [SQUARE_METRE]
    NetSideArea = 67.12 [SQUARE_METRE]
    NetVolume = 6.24 [CUBIC_METRE]
    NetVolume = 6240000000. [CUBIC_METRE]
    Width = 200. [MILLI METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCDOOR)
    Area = 3.18957899999998 [SQUARE_METRE]
    Height = 2134. [MILLI METRE]
    Width = 915. [MILLI METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.760000000000001 [SQUARE_METRE]
    Height = 4000. [MILLI METRE]
    Length = 3800.00000000001 [MILLI METRE]
    NetSideArea = 15200000. [SQUARE_METRE]
    NetSideArea = 33.5200000000001 [SQUARE_METRE]
    NetVolume = 3.04000000000001 [CUBIC_METRE]
    NetVolume = 3040000000.00001 [CUBIC_METRE]
    Width = 200. [MILLI METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCOPENINGELEMENT)
    Depth = 200. [MILLI METRE]
    Height = 915. [MILLI METRE]
    Width = 2134. [MILLI METRE]
  BaseQuantities | quantities | on 3 objects (3 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 1.64000000000001 [SQUARE_METRE]
    Height = 4000. [MILLI METRE]
    Length = 8200.00000000003 [MILLI METRE]
    NetSideArea = 32800000.0000001 [SQUARE_METRE]
    NetSideArea = 65.9782000000003 [SQUARE_METRE]
    NetVolume = 5.89022000000003 [CUBIC_METRE]
    NetVolume = 6560000000.00003 [CUBIC_METRE]
    Width = 200. [MILLI METRE]
  BaseQuantities | quantities | on 3 objects (3 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 1.6 [SQUARE_METRE]
    Height = 4000. [MILLI METRE]
    Length = 8000. [MILLI METRE]
    NetSideArea = 32000000. [SQUARE_METRE]
    NetSideArea = 68.8 [SQUARE_METRE]
    NetVolume = 6.4 [CUBIC_METRE]
    NetVolume = 6400000000. [CUBIC_METRE]
    Width = 200. [MILLI METRE]
  BaseQuantities: 17 more contents on 20 objects not shown
  Constraints | properties | on 24 objects (24 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Cross-Section = "Vertical" (IFCIDENTIFIER)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: Level 6" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 16000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 7 objects (7 IFCWINDOW)
    Level = "Level: Level 2" (IFCLABEL)
    Sill Height = 305.000000000004 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 6 objects (6 IFCWINDOW)
    Level = "Level: Level 1" (IFCLABEL)
    Sill Height = 305.000000000004 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 5 objects (5 IFCDOOR)
    Level = "Level: Level 1" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 4 objects (4 IFCWINDOW)
    Level = "Level: Level 4" (IFCLABEL)
    Sill Height = 305.000000000005 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 4 objects (4 IFCWINDOW)
    Level = "Level: Level 5" (IFCLABEL)
    Sill Height = 305.000000000005 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 3 objects (3 IFCSPACE)
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level 1" (IFCTEXT)
    Limit Offset = 4000. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Limit = "Level: Level 1" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCSLAB)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: Level 1" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints: 9 more contents on 9 objects not shown
  Dimensions | properties | on 21 objects (21 IFCWINDOW)
    Area = 3.17875400000013 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0561146700000025 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Area = 116.574400000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 23.3148800000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Area = 122.89478 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 24.578956 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Area = 113.404400000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 8000.00000000004 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 22.6808800000002 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Area = 112.119 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 22.4238 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 4 objects (4 IFCDOOR)
    Area = 3.18957899999998 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.119856109999999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Area = 120.89478 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 24.178956 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 12 more contents on 13 objects not shown
  Energy Analysis | properties | on 3 objects (3 IFCSPACE)
    Actual Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Lighting Load per area = 0. (IFCREAL)
    Actual Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Power Load per area = 0. (IFCREAL)
    Area per Person = 28.5714285714286 (IFCAREAMEASURE) [SQUARE_METRE]
    Base Lighting Load on = "By Space Type" (IFCIDENTIFIER)
    Base Power Load on = "By Space Type" (IFCIDENTIFIER)
    Heat Load Values = "By Space Type" (IFCIDENTIFIER)
    Latent Heat Gain per person = 58.6142140344444 (IFCPOWERMEASURE) [WATT]
    Lighting Load Units = "Power Density" (IFCIDENTIFIER)
    Number of People = 0. (IFCREAL)
    Plenum Lighting Contribution = 20. (IFCREAL)
    Power Load Units = "Power Density" (IFCIDENTIFIER)
    Sensible Heat Gain per person = 73.2677675430556 (IFCPOWERMEASURE) [WATT]
    Specified Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Specified Lighting Load per area = 10.7639104167097 (IFCREAL)
    Specified Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Specified Power Load per area = 13.9930835417226 (IFCREAL)
    Total Heat Gain per person = 131.8819815775 (IFCPOWERMEASURE) [WATT]
  Phasing | properties | on 55 objects (24 IFCWALLSTANDARDCASE, 21 IFCWINDOW, 5 IFCDOOR, 4 IFCSLAB)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 3 objects (3 IFCSPACE)
    Phase = "New Construction" (IFCLABEL)
  Structural | properties | on 24 objects (24 IFCWALLSTANDARDCASE)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Structural | properties | on 4 objects (4 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Pset_ConcreteElementGeneral | properties | on 24 objects (24 IFCWALLSTANDARDCASE) | on 2 type objects
    FireRating = "_FIRE-RATING_" (IFCLABEL)
  Pset_ConcreteElementGeneral | properties | on 2 objects (2 IFCDOOR) | on 2 type objects
    FireRating = "Inside door: Fire Rating" (IFCLABEL)
  Pset_ConcreteElementGeneral | properties | on 2 objects (2 IFCDOOR) | on 1 type object
    FireRating = "--FIRE_CODE--" (IFCLABEL)
  Pset_ConcreteElementGeneral | properties | on 1 object (1 IFCDOOR) | on 1 type object
    FireRating = "Special wall: Fire Rating" (IFCLABEL)
  Pset_ElementShading | properties | on 30 objects (24 IFCWALLSTANDARDCASE, 5 IFCSLAB, 1 IFCROOF) | on 6 type objects
    Roughness = 914.4 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ManufacturerTypeInformation | properties | on 24 objects (24 IFCWALLSTANDARDCASE) | on 2 type objects
    Manufacturer = "_MANUFACTURER_" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 21 objects (21 IFCWINDOW) | on 1 type object
    Manufacturer = "Window: Manufacturer" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCDOOR) | on 2 type objects
    Manufacturer = "Inside door: Manufacturer" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCDOOR) | on 1 type object
    Manufacturer = "--TYPE_COMMENTS_" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Manufacturer = "Special wall: Manufacturer" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 21 objects (21 IFCWINDOW) | on 1 type object
    Reference = "0915 x 1830mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 16 objects (16 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Outside wall" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 8 objects (8 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Inside" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCSLAB) | on 4 type objects
    Reference = "Generic 150mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCDOOR) | on 2 type objects
    Reference = "Inside Door" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCDOOR) | on 1 type object
    Reference = "Outside door" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "Generic - 400mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Reference = "1500 x 2000mm" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 16 objects (16 IFCWALLSTANDARDCASE) | on 1 type object
    Description = "_DESCRIPTION_" (IFCTEXT)
    Reference = "Outside wall" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 8 objects (8 IFCWALLSTANDARDCASE) | on 1 type object
    Description = "_DESCRIPTION_" (IFCTEXT)
    Reference = "Inside" (IFCLABEL)
  Pset_WallCommon | properties | on 16 objects (16 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "_FIRE-RATING_" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Outside wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 8 objects (8 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "_FIRE-RATING_" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Inside" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    FireRating = "_FIRE-RATING_" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Outside wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    FireRating = "_FIRE-RATING_" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Inside" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR) | on 2 type objects
    FireRating = "Inside door: Fire Rating" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Inside Door" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR) | on 1 type object
    FireRating = "--FIRE_CODE--" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Outside door" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR) | on 1 type object
    FireRating = "Special wall: Fire Rating" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1500 x 2000mm" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCDOOR)
    Swing Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 16400. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
    Rafter or Truss = "Truss" (IFCIDENTIFIER)
  Construction | properties | on 4 type objects
    Function = "Interior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Construction | properties | on 4 type objects
    Default Thickness = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Construction | properties | on 2 type objects
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Wall Closure = "By host" (IFCIDENTIFIER)
  Graphics | properties | on 1 object (1 IFCDOOR)
    Show Grill = TRUE (IFCBOOLEAN)
  Graphics | properties | on 6 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Pset_WindowCommon | properties | on 21 objects (21 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0915 x 1830mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 1830mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ReinforcementBarPitchOfSlab | properties | on 4 objects (4 IFCSLAB) | on 4 type objects
    Reference = "Generic 150mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Generic - 400mm" (IFCLABEL)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Generic 150mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Generic - 400mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 4 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic 150mm" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 67.2400000000003 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Generic - 400mm" (IFCIDENTIFIER)
    TotalArea = 67.2400000000003 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_BuildingStoreyCommon | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 5 (IFCINTEGER)
  Constraints(Type) | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Other(Type) | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Analytical Properties | properties | on 6 type objects
    Absorptance = 0.7 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
  Analytical Properties | properties | on 3 type objects
    Analytic Construction = "Metal" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
    Heat Transfer Coefficient (U) = 3.7021 (IFCREAL)
    Solar Heat Gain Coefficient = 0. (IFCREAL)
    Thermal Resistance (R) = 0.270116960643959 (IFCREAL)
    Visual Light Transmittance = 0. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "1/8 in Pilkington single glazing" (IFCTEXT)
    Define Thermal Properties by = "Schematic Type" (IFCIDENTIFIER)
    Heat Transfer Coefficient (U) = 3.6886 (IFCREAL)
    Solar Heat Gain Coefficient = 0.78 (IFCREAL)
    Thermal Resistance (R) = 0.271105568508377 (IFCREAL)
    Visual Light Transmittance = 0.9 (IFCREAL)
  M_Door-Interior-Double-Full Glass-Wood:1500 x 2000mm:358703 | predefined | on 2 type objects
  Materials and Finishes | properties | on 3 type objects
    Door Material = "Door - Panel" (IFCLABEL)
    Frame Material = "Door - Frame" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Door Handle Material = "Aluminum" (IFCLABEL)
    Frame Material = "Cherry" (IFCLABEL)
    Panel Material = "Cherry" (IFCLABEL)
    Trim Material = "Cherry" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Frame Exterior Material = "Sash" (IFCLABEL)
    Frame Interior Material = "Sash" (IFCLABEL)
    Glass Pane Material = "Glass" (IFCLABEL)
    Sash = "Sash" (IFCLABEL)
  M_Single-Flush:Outside door:358883 | predefined | on 2 type objects
  M_Single-Flush:Inside Door:359375 | predefined | on 2 type objects
  M_Single-Flush:Inside Door:359428 | predefined | on 2 type objects
  M_Fixed:0915 x 1830mm:359493 | predefined | on 1 type object