IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
Description: "RevitIdentifiers [ContentGUID: 890f9267-8c55-4fd2-bfe7-ed6d35141e7e, VersionGUID: 21700bc6-4038-4c54-8245-a02c80ec9c57, NumberOfSaves: 21]"
File name: "input__{3D}.ifc"
Time stamp: "2025-12-03T15:37:36-00:00"
Preprocessor: "ODA SDAI 24.12"
Originating system: "Autodesk Revit 25.3.0.46 (ENU) - IFC 25.3.0.46"
Application: "Autodesk Revit 2025 (ENU)" version "2025" identifier "Revit" by Organization "Autodesk Revit 2025 (ENU)"

People and organizations
  Person "acesuser" of Organization (no name given)
  Owner history of Person "acesuser" of Organization (no name given) | application "Autodesk Revit 2025 (ENU)" version "2025" identifier "Revit" by Organization "Autodesk Revit 2025 (ENU)" | change NOCHANGE | created 1764776194 (2025-12-03T15:36:34Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  THERMALTRANSMITTANCEUNIT: derived
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT "001-00" | long name "Sample House" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 23′ 13.199999″ | longitude -71° 14′ 31.199999″ | elevation above sea level 0.
    contains 615 elements
      9 x IFCWALL | type IFCWALLTYPE "Basic Wall:CL_W1" | object type "Basic Wall:CL_W1" | names: "Basic Wall:CL_W1:493612", "Basic Wall:CL_W1:493879", "Basic Wall:CL_W1:627064" (+6 more) | material: layers "Basic Wall:CL_W1" ("CL Concrete_ panels" 280.) | property sets: Qto_WallBaseQuantities, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
      2 x IFCSLAB | type IFCSLABTYPE "Floor:Insitu Concrete" | object type "Floor:Insitu Concrete" | FLOOR | names: "Floor:Insitu Concrete:495352", "Floor:Insitu Concrete:1206619" | material: layers "Floor:Insitu Concrete" ("Concrete - Cast-in-Place Concrete" 50., "Concrete - Rough" 200., "Rigid insulation" 100., "Damp-proofing" 0., "Rubble" 200.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Qto_SlabBaseQuantities
      8 x IFCSLAB | type IFCSLABTYPE "M_Pile Cap-600 Pile:600 x 600 x 900mm" | object type "M_Pile Cap-600 Pile:600 x 600 x 900mm" | BASESLAB | names: "M_Pile Cap-600 Pile:600 x 600 x 900mm:512319", "M_Pile Cap-600 Pile:600 x 600 x 900mm:512394", "M_Pile Cap-600 Pile:600 x 600 x 900mm:512445" (+5 more) | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Qto_SlabBaseQuantities
      17 x IFCSLAB | type IFCSLABTYPE "M_Pile-Steel Pipe:600mm Diameter" | object type "M_Pile-Steel Pipe:600mm Diameter" | BASESLAB | names: "M_Pile-Steel Pipe:600mm Diameter:512321", "M_Pile-Steel Pipe:600mm Diameter:512396", "M_Pile-Steel Pipe:600mm Diameter:512447" (+14 more) | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Qto_SlabBaseQuantities
      1 x IFCSTAIR | type IFCSTAIRTYPE "Assembled Stair:190mm max riser 250mm going" | object type "Assembled Stair:190mm max riser 250mm going" | STRAIGHT_RUN_STAIR | names: "Assembled Stair:Stair:513254" | parts: 2 IFCMEMBER, 1 IFCSTAIRFLIGHT | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
      1 x IFCSLAB | type IFCSLABTYPE "Floor:Insitu Concrete 250mm" | object type "Floor:Insitu Concrete 250mm" | FLOOR | names: "Floor:Insitu Concrete 250mm:647908" | material: layers "Floor:Insitu Concrete 250mm" ("Concrete - Cast-in-Place Concrete" 50., "Concrete - Rough" 200., "Damp-proofing" 0., "Rubble" 200.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Qto_SlabBaseQuantities
      4 x IFCCOLUMN | type IFCCOLUMNTYPE "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | object type "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | COLUMN | names: "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1046264", "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1096413", "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1436414" (+1 more) | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1046268" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      9 x IFCBEAM | type IFCBEAMTYPE "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | object type "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | BEAM | names: "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS:1046278", "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS:1046281", "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS:1046284" (+6 more) | material: profiles "88.9x5.0CHS" ("88.9x5.0CHS": "Metal Stud Layer") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      72 x IFCMEMBER | type IFCMEMBERTYPE "Light Gauge-Joists:SC15012" | object type "Light Gauge-Joists:SC15012" | PURLIN | names: "Light Gauge-Joists:SC15012:1046298", "Light Gauge-Joists:SC15012:1046300", "Light Gauge-Joists:SC15012:1046302" (+69 more) | material: profiles "SC15012" ("SC15012": "Aluminum") | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities
      16 x IFCMEMBER | type IFCMEMBERTYPE "Light Gauge-Joists:SC15012" | object type "Light Gauge-Joists:SC15012" | PURLIN | names: "Light Gauge-Joists:SC15012:1046306", "Light Gauge-Joists:SC15012:1046318", "Light Gauge-Joists:SC15012:1046330" (+13 more) | material: profiles "SC15012" ("SC15012": "Aluminum") | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities
      4 x IFCMEMBER | type IFCMEMBERTYPE "Light Gauge-Joists:SC15012" | object type "Light Gauge-Joists:SC15012" | PURLIN | names: "Light Gauge-Joists:SC15012:1046346", "Light Gauge-Joists:SC15012:1046352", "Light Gauge-Joists:SC15012:1046490" (+1 more) | material: profiles "SC15012" ("SC15012": "Aluminum") | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities
      4 x IFCMEMBER | type IFCMEMBERTYPE "Light Gauge-Joists:SC15012" | object type "Light Gauge-Joists:SC15012" | PURLIN | names: "Light Gauge-Joists:SC15012:1046382", "Light Gauge-Joists:SC15012:1046388", "Light Gauge-Joists:SC15012:1046442" (+1 more) | material: profiles "SC15012" ("SC15012": "Aluminum") | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities
      6 x IFCMEMBER | type IFCMEMBERTYPE "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | object type "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | PURLIN | names: "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS:1046392", "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS:1046394", "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS:1046396" (+3 more) | material: profiles "88.9x5.0CHS" ("88.9x5.0CHS": "Metal Stud Layer") | property sets: Pset_EnvironmentalImpactIndicators, Pset_MemberCommon, Qto_MemberBaseQuantities
      2 x IFCBEAM | type IFCBEAMTYPE "Round Bar:30mm" | object type "Round Bar:30mm" | BEAM | names: "Round Bar:30mm:1046542", "Round Bar:30mm:1046558" | material: profiles "30mm" ("30mm": "Metal Stud Layer") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      4 x IFCBEAM | type IFCBEAMTYPE "Round Bar:30mm" | object type "Round Bar:30mm" | BEAM | names: "Round Bar:30mm:1046544", "Round Bar:30mm:1046550", "Round Bar:30mm:1046560" (+1 more) | material: profiles "30mm" ("30mm": "Metal Stud Layer") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      2 x IFCBEAM | type IFCBEAMTYPE "Round Bar:30mm" | object type "Round Bar:30mm" | BEAM | names: "Round Bar:30mm:1046546", "Round Bar:30mm:1046562" | material: profiles "30mm" ("30mm": "Metal Stud Layer") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      4 x IFCBEAM | type IFCBEAMTYPE "Round Bar:30mm" | object type "Round Bar:30mm" | BEAM | names: "Round Bar:30mm:1046548", "Round Bar:30mm:1046554", "Round Bar:30mm:1046564" (+1 more) | material: profiles "30mm" ("30mm": "Metal Stud Layer") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      2 x IFCBEAM | type IFCBEAMTYPE "Round Bar:30mm" | object type "Round Bar:30mm" | BEAM | names: "Round Bar:30mm:1046552", "Round Bar:30mm:1046568" | material: profiles "30mm" ("30mm": "Metal Stud Layer") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      2 x IFCBEAM | type IFCBEAMTYPE "Round Bar:30mm" | object type "Round Bar:30mm" | BEAM | names: "Round Bar:30mm:1046556", "Round Bar:30mm:1046572" | material: profiles "30mm" ("30mm": "Metal Stud Layer") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      4 x IFCCOLUMN | type IFCCOLUMNTYPE "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | object type "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | COLUMN | names: "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1096385", "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1096419", "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1436418" (+1 more) | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1096387" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1096415" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1096421" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      3 x IFCCOLUMN | type IFCCOLUMNTYPE "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | object type "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | COLUMN | names: "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1098642", "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1436859", "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1436901" | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1098644" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      3 x IFCCOLUMN | type IFCCOLUMNTYPE "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | object type "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | COLUMN | names: "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1114995", "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1436688", "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1436726" | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1114997" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1116436" | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      4 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1116461", "UB-Universal Beams (AS 3679_1):200UB25.4:1117306", "UB-Universal Beams (AS 3679_1):200UB25.4:1175513" (+1 more) | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1116483" | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1116502" | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      4 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1116979", "UB-Universal Beams (AS 3679_1):200UB25.4:1117017", "UB-Universal Beams (AS 3679_1):200UB25.4:1117037" (+1 more) | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Square-Column:450 x 450mm" | object type "M_Concrete-Square-Column:450 x 450mm" | COLUMN | names: "M_Concrete-Square-Column:450 x 450mm:1173925" | material: profiles "450 x 450mm" ("450 x 450mm": "Concrete, Cast-in-Place gray") | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1174038" | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCSLAB | type IFCSLABTYPE "Pile Cap-9 Pile:3800 x 3800 x 600mm" | object type "Pile Cap-9 Pile:3800 x 3800 x 600mm" | BASESLAB | names: "Pile Cap-9 Pile:3800 x 3800 x 600mm:1175183" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Qto_SlabBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1175555" | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1175999" | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      2 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1176035", "UB-Universal Beams (AS 3679_1):200UB25.4:1176046" | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1176054" | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      4 x IFCFOOTING | type IFCFOOTINGTYPE "Wall Foundation:Bearing Footing - 900 x 300" | object type "Wall Foundation:Bearing Footing - 900 x 300" | STRIP_FOOTING | names: "Wall Foundation:Bearing Footing - 900 x 300:1178019", "Wall Foundation:Bearing Footing - 900 x 300:1178029", "Wall Foundation:Bearing Footing - 900 x 300:1178049" (+1 more) | material: "Concrete - Cast-in-Place Concrete - 35 MPa" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FootingCommon, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting, Qto_FootingBaseQuantities
      1 x IFCSLAB | type IFCSLABTYPE "Floor:Plywood double brace" | object type "Floor:Plywood double brace" | FLOOR | names: "Floor:Plywood double brace:1210630" | material: layers "Floor:Plywood double brace" ("Plywood, Sheathing" 22., "Plywood, Sheathing" 22.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Qto_SlabBaseQuantities
      1 x IFCSLAB | type IFCSLABTYPE "Floor:Rigid Insulation" | object type "Floor:Rigid Insulation" | FLOOR | names: "Floor:Rigid Insulation:1211070" | material: layers "Floor:Rigid Insulation" ("Rigid insulation" 100.) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Qto_SlabBaseQuantities
      334 x IFCREINFORCINGBAR | type IFCREINFORCINGBARTYPE "Rebar Bar:Structural Rebar 1" | object type "Rebar Bar:Structural Rebar 1" | names: "Rebar Bar:Structural Rebar 1:1316567", "Rebar Bar:Structural Rebar 1:1316568", "Rebar Bar:Structural Rebar 1:1316569" (+331 more) | property sets: Pset_ElementComponentCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcingBarCommon
      6 x IFCSLAB | type IFCSLABTYPE "Pile Cap-Rectangular:400 x 400 x 900mm" | object type "Pile Cap-Rectangular:400 x 400 x 900mm" | BASESLAB | names: "Pile Cap-Rectangular:400 x 400 x 900mm:1381249", "Pile Cap-Rectangular:400 x 400 x 900mm:1381270", "Pile Cap-Rectangular:400 x 400 x 900mm:1381287" (+3 more) | material: "Concrete, Cast-in-Place gray" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Qto_SlabBaseQuantities
      12 x IFCREINFORCINGBAR | type IFCREINFORCINGBARTYPE "Rebar Bar:Structural Rebar 12mm" | object type "Rebar Bar:Structural Rebar 12mm" | names: "Rebar Bar:Structural Rebar 12mm : Shape Rebar Shape 4:1381252", "Rebar Bar:Structural Rebar 12mm : Shape Rebar Shape 4:1381255", "Rebar Bar:Structural Rebar 12mm : Shape Rebar Shape 4:1381273" (+9 more) | property sets: Pset_ElementComponentCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcingBarCommon
      4 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1417275", "UB-Universal Beams (AS 3679_1):200UB25.4:1417277", "UB-Universal Beams (AS 3679_1):200UB25.4:1417279" (+1 more) | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      12 x IFCCOLUMN | type IFCCOLUMNTYPE "M_HSS Square-Column:HSS63.5X63.5X7.9" | object type "M_HSS Square-Column:HSS63.5X63.5X7.9" | COLUMN | names: "M_HSS Square-Column:HSS63.5X63.5X7.9:1417448", "M_HSS Square-Column:HSS63.5X63.5X7.9:1417450", "M_HSS Square-Column:HSS63.5X63.5X7.9:1417452" (+9 more) | material: profiles "HSS63.5X63.5X7.9" ("HSS63.5X63.5X7.9": "Steel, 45-345") | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
      1 x IFCBEAM | type IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | object type "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | names: "PFC-Parallel Flange Channels (AS 3679_1):200PFC:1417462" | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | object type "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | names: "PFC-Parallel Flange Channels (AS 3679_1):200PFC:1417464" | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | object type "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | names: "PFC-Parallel Flange Channels (AS 3679_1):200PFC:1417466" | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | object type "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | names: "PFC-Parallel Flange Channels (AS 3679_1):200PFC:1417469" | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | object type "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | names: "PFC-Parallel Flange Channels (AS 3679_1):200PFC:1417471" | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | object type "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | names: "PFC-Parallel Flange Channels (AS 3679_1):200PFC:1417473" | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | object type "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | names: "PFC-Parallel Flange Channels (AS 3679_1):200PFC:1417487" | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      3 x IFCCOLUMN | type IFCCOLUMNTYPE "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | object type "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | COLUMN | names: "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1432709", "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1436866", "UB-Universal Beams-Column (AS 3679_1):200UB25.4:1436907" | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1436416" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1436420" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1436523" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1436528" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1436690" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1436728" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1436861" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | object type "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | names: "UB-Universal Beams (AS 3679_1):200UB25.4:1436903" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | object type "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | BEAM | names: "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS:1437055" | material: profiles "88.9x5.0CHS" ("88.9x5.0CHS": "Metal Stud Layer") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | object type "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | BEAM | names: "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS:1437083" | material: profiles "88.9x5.0CHS" ("88.9x5.0CHS": "Metal Stud Layer") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      1 x IFCBEAM | type IFCBEAMTYPE "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | object type "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | BEAM | names: "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS:1437167" | material: profiles "88.9x5.0CHS" ("88.9x5.0CHS": "Metal Stud Layer") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
      16 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Beam System:Structural Framing System:1175801", "Structural Beam System:Structural Framing System:1175865", "Structural Beam System:Structural Framing System:1175908" (+13 more) | parts: 198 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators

Types
  IFCWALLTYPE "Basic Wall:CL_W1" | STANDARD | 9 occurrences | material: layers "Basic Wall:CL_W1" ("CL Concrete_ panels" 280.) | property sets: Pset_WallCommon
  IFCSLABTYPE "Floor:Insitu Concrete" | FLOOR | 2 occurrences | material: layers "Floor:Insitu Concrete" ("Concrete - Cast-in-Place Concrete" 50., "Concrete - Rough" 200., "Rigid insulation" 100., "Damp-proofing" 0., "Rubble" 200.) | property sets: Pset_SlabCommon
  IFCSLABTYPE "M_Pile Cap-600 Pile:600 x 600 x 900mm" | BASESLAB | 8 occurrences | material: "Concrete - Cast-in-Place Concrete"
  IFCSLABTYPE "M_Pile-Steel Pipe:600mm Diameter" | BASESLAB | 17 occurrences | material: "Concrete - Cast-in-Place Concrete"
  IFCSTAIRTYPE "Assembled Stair:190mm max riser 250mm going" | STRAIGHT_RUN_STAIR | 1 occurrence | property sets: Pset_StairCommon, Pset_StairFlightCommon
  IFCSLABTYPE "Floor:Insitu Concrete 250mm" | FLOOR | 1 occurrence | material: layers "Floor:Insitu Concrete 250mm" ("Concrete - Cast-in-Place Concrete" 50., "Concrete - Rough" 200., "Damp-proofing" 0., "Rubble" 200.) | property sets: Pset_SlabCommon
  IFCCOLUMNTYPE "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | COLUMN | 4 occurrences | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | BEAM | 9 occurrences | material: profiles "88.9x5.0CHS" ("88.9x5.0CHS": "Metal Stud Layer") | property sets: Pset_BeamCommon
  IFCMEMBERTYPE "Light Gauge-Joists:SC15012" | PURLIN | 72 occurrences | material: profiles "SC15012" ("SC15012": "Aluminum") | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "Light Gauge-Joists:SC15012" | PURLIN | 16 occurrences | material: profiles "SC15012" ("SC15012": "Aluminum") | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "Light Gauge-Joists:SC15012" | PURLIN | 4 occurrences | material: profiles "SC15012" ("SC15012": "Aluminum") | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "Light Gauge-Joists:SC15012" | PURLIN | 4 occurrences | material: profiles "SC15012" ("SC15012": "Aluminum") | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | PURLIN | 6 occurrences | material: profiles "88.9x5.0CHS" ("88.9x5.0CHS": "Metal Stud Layer") | property sets: Pset_MemberCommon
  IFCBEAMTYPE "Round Bar:30mm" | BEAM | 2 occurrences | material: profiles "30mm" ("30mm": "Metal Stud Layer") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Round Bar:30mm" | BEAM | 4 occurrences | material: profiles "30mm" ("30mm": "Metal Stud Layer") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Round Bar:30mm" | BEAM | 2 occurrences | material: profiles "30mm" ("30mm": "Metal Stud Layer") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Round Bar:30mm" | BEAM | 4 occurrences | material: profiles "30mm" ("30mm": "Metal Stud Layer") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Round Bar:30mm" | BEAM | 2 occurrences | material: profiles "30mm" ("30mm": "Metal Stud Layer") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Round Bar:30mm" | BEAM | 2 occurrences | material: profiles "30mm" ("30mm": "Metal Stud Layer") | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | COLUMN | 4 occurrences | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | COLUMN | 3 occurrences | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | COLUMN | 3 occurrences | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 4 occurrences | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 4 occurrences | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "M_Concrete-Square-Column:450 x 450mm" | COLUMN | 1 occurrence | material: profiles "450 x 450mm" ("450 x 450mm": "Concrete, Cast-in-Place gray") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCSLABTYPE "Pile Cap-9 Pile:3800 x 3800 x 600mm" | BASESLAB | 1 occurrence | material: "Concrete - Cast-in-Place Concrete"
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 2 occurrences | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCFOOTINGTYPE "Wall Foundation:Bearing Footing - 900 x 300" | STRIP_FOOTING | 4 occurrences
  IFCSLABTYPE "Floor:Plywood double brace" | FLOOR | 1 occurrence | material: layers "Floor:Plywood double brace" ("Plywood, Sheathing" 22., "Plywood, Sheathing" 22.) | property sets: Pset_SlabCommon
  IFCSLABTYPE "Floor:Rigid Insulation" | FLOOR | 1 occurrence | material: layers "Floor:Rigid Insulation" ("Rigid insulation" 100.) | property sets: Pset_SlabCommon
  IFCREINFORCINGBARTYPE "Rebar Bar:Structural Rebar 1" | 334 occurrences
  IFCSLABTYPE "Pile Cap-Rectangular:400 x 400 x 900mm" | BASESLAB | 6 occurrences | material: "Concrete, Cast-in-Place gray"
  IFCREINFORCINGBARTYPE "Rebar Bar:Structural Rebar 12mm" | 12 occurrences
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 4 occurrences | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "M_HSS Square-Column:HSS63.5X63.5X7.9" | COLUMN | 12 occurrences | material: profiles "HSS63.5X63.5X7.9" ("HSS63.5X63.5X7.9": "Steel, 45-345") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | 1 occurrence | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | 1 occurrence | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | 1 occurrence | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | 1 occurrence | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | 1 occurrence | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | 1 occurrence | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "PFC-Parallel Flange Channels (AS 3679_1):200PFC" | BEAM | 1 occurrence | material: profiles "200PFC" ("200PFC": "Metal - Steel - 250 MPa") | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "UB-Universal Beams-Column (AS 3679_1):200UB25.4" | COLUMN | 3 occurrences | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "UB-Universal Beams (AS 3679_1):200UB25.4" | BEAM | 1 occurrence | material: profiles "200UB25.4" ("200UB25.4": "Metal - Steel - 345 MPa") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | BEAM | 1 occurrence | material: profiles "88.9x5.0CHS" ("88.9x5.0CHS": "Metal Stud Layer") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | BEAM | 1 occurrence | material: profiles "88.9x5.0CHS" ("88.9x5.0CHS": "Metal Stud Layer") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "CHS-Circular Hollow Sections (AS 1163_C250L0):88.9x5.0CHS" | BEAM | 1 occurrence | material: profiles "88.9x5.0CHS" ("88.9x5.0CHS": "Metal Stud Layer") | property sets: Pset_BeamCommon

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.6958679999999879 [SQUARE_METRE]
    GrossSideArea = 45.252069999999577 [SQUARE_METRE]
    GrossVolume = 12.670579599999883 [CUBIC_METRE]
    Height = 4700. [MILLI METRE]
    Length = 9628.0999999999112 [MILLI METRE]
    NetSideArea = 45.252069999999577 [SQUARE_METRE]
    NetVolume = 12.670579599999845 [CUBIC_METRE]
    Width = 280. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.1374285200016989 [SQUARE_METRE]
    GrossSideArea = 37.84238067549709 [SQUARE_METRE]
    GrossVolume = 10.595866589139185 [CUBIC_METRE]
    Height = 4700. [MILLI METRE]
    Length = 8051.5703564887417 [MILLI METRE]
    NetSideArea = 37.84238067549709 [SQUARE_METRE]
    NetVolume = 10.045914044007986 [CUBIC_METRE]
    Width = 280. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 6.8348000000000084 [SQUARE_METRE]
    GrossSideArea = 29.292000000000009 [SQUARE_METRE]
    GrossVolume = 8.2017600000000037 [CUBIC_METRE]
    Height = 1200. [MILLI METRE]
    Length = 24410.000000000007 [MILLI METRE]
    NetSideArea = 29.292000000000012 [SQUARE_METRE]
    NetVolume = 8.2017600000000073 [CUBIC_METRE]
    Width = 280. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.8514611442000251 [SQUARE_METRE]
    GrossSideArea = 8.0616274421572207 [SQUARE_METRE]
    GrossVolume = 2.2572556838040216 [CUBIC_METRE]
    Height = 1200. [MILLI METRE]
    Length = 6718.0228684643489 [MILLI METRE]
    NetSideArea = 8.0616274421572189 [SQUARE_METRE]
    NetVolume = 2.2217533730400332 [CUBIC_METRE]
    Width = 280. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 6.1552399999999912 [SQUARE_METRE]
    GrossSideArea = 26.379599999999943 [SQUARE_METRE]
    GrossVolume = 7.3862879999999844 [CUBIC_METRE]
    Height = 1200. [MILLI METRE]
    Length = 21982.999999999953 [MILLI METRE]
    NetSideArea = 26.379599999999947 [SQUARE_METRE]
    NetVolume = 7.3862879999999889 [CUBIC_METRE]
    Width = 280. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.25200000000015199 [SQUARE_METRE]
    GrossSideArea = 1.0800000000006467 [SQUARE_METRE]
    GrossVolume = 0.30240000000018108 [CUBIC_METRE]
    Height = 1200. [MILLI METRE]
    Length = 900.00000000053876 [MILLI METRE]
    NetSideArea = 1.0800000000006467 [SQUARE_METRE]
    NetVolume = 0.30240000000017958 [CUBIC_METRE]
    Width = 280. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 0.75796000000002617 [SQUARE_METRE]
    GrossSideArea = 3.248400000000109 [SQUARE_METRE]
    GrossVolume = 0.90955200000003045 [CUBIC_METRE]
    Height = 1200. [MILLI METRE]
    Length = 2707.0000000000905 [MILLI METRE]
    NetSideArea = 3.248400000000109 [SQUARE_METRE]
    NetVolume = 0.90955200000003156 [CUBIC_METRE]
    Width = 280. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 5.9131425452192836 [SQUARE_METRE]
    GrossSideArea = 100.12816088304741 [SQUARE_METRE]
    GrossVolume = 28.035885047253277 [CUBIC_METRE]
    Height = 4700. [MILLI METRE]
    Length = 21303.864017669661 [MILLI METRE]
    NetSideArea = 100.12816088304739 [SQUARE_METRE]
    NetVolume = 27.791769962530648 [CUBIC_METRE]
    Width = 280. [MILLI METRE]
  Qto_WallBaseQuantities: 1 more content on 1 objects not shown
  Pset_EnvironmentalImpactIndicators | properties | on 334 objects (334 IFCREINFORCINGBAR)
    Reference = "Structural Rebar 1" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 106 objects (106 IFCBEAM)
    Reference = "Timber_50 x200" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 96 objects (96 IFCMEMBER)
    Reference = "SC15012" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 65 objects (65 IFCBEAM)
    Reference = "Timber_50 x150 _ContentGenerator" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 52 objects (35 IFCBEAM, 17 IFCCOLUMN)
    Reference = "200UB25.4" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 27 objects (27 IFCBEAM)
    Reference = "356mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 18 objects (12 IFCBEAM, 6 IFCMEMBER)
    Reference = "88.9x5.0CHS" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 17 objects (17 IFCSLAB)
    Reference = "600mm Diameter" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators: 18 more contents on 101 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 9 objects (9 IFCWALL)
    Reference = "CL_W1" (IFCLABEL)
  Pset_WallCommon | properties | on 7 objects (7 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "CL_W1" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "CL_W1" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    ThermalTransmittance = 0.75 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ReinforcementBarPitchOfSlab | properties | on 17 objects (17 IFCSLAB)
    Reference = "600mm Diameter" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 8 objects (8 IFCSLAB)
    Reference = "600 x 600 x 900mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 6 objects (6 IFCSLAB)
    Reference = "400 x 400 x 900mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Insitu Concrete" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Insitu Concrete 250mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "3800 x 3800 x 600mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Plywood double brace" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Rigid Insulation" (IFCLABEL)
  Pset_SlabCommon | properties | on 17 objects (17 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "600mm Diameter" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 8 objects (8 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "600 x 600 x 900mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 6 objects (6 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "400 x 400 x 900mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Insitu Concrete" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Insitu Concrete 250mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "3800 x 3800 x 600mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Plywood double brace" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Rigid Insulation" (IFCIDENTIFIER)
  Pset_SlabCommon: 4 more contents on 0 objects not shown
  Qto_SlabBaseQuantities | quantities | on 4 objects (4 IFCSLAB)
    Depth = 900.00000000000011 [MILLI METRE]
    GrossArea = 0.16 [SQUARE_METRE]
    GrossVolume = 0.14400000000000002 [CUBIC_METRE]
    Length = 400. [MILLI METRE]
    NetArea = 0.16 [SQUARE_METRE]
    NetVolume = 0.14399999999999982 [CUBIC_METRE]
    Perimeter = 1600. [MILLI METRE]
    Width = 400. [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 3 objects (3 IFCSLAB)
    Depth = 299.99999999999989 [MILLI METRE]
    GrossArea = 0.36000000000000004 [SQUARE_METRE]
    GrossVolume = 0.10799999999999997 [CUBIC_METRE]
    Length = 600. [MILLI METRE]
    NetArea = 0.35999999999999999 [SQUARE_METRE]
    NetVolume = 0.1079999999999999 [CUBIC_METRE]
    Perimeter = 2400. [MILLI METRE]
    Width = 600. [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 3 objects (3 IFCSLAB)
    Depth = 6000. [MILLI METRE]
    GrossArea = 0.070673092907964932 [SQUARE_METRE]
    NetArea = 0.070673092907964932 [SQUARE_METRE]
    NetVolume = 0.42423381306804264 [CUBIC_METRE]
  Qto_SlabBaseQuantities | quantities | on 2 objects (2 IFCSLAB)
    Depth = 299.99999999999989 [MILLI METRE]
    GrossArea = 0.35999999999999999 [SQUARE_METRE]
    GrossVolume = 0.10799999999999996 [CUBIC_METRE]
    Length = 600. [MILLI METRE]
    NetArea = 0.35999999999999999 [SQUARE_METRE]
    NetVolume = 0.10799999999999996 [CUBIC_METRE]
    Perimeter = 2400. [MILLI METRE]
    Width = 600. [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 2 objects (2 IFCSLAB)
    Depth = 6000. [MILLI METRE]
    GrossArea = 0.070673092907964932 [SQUARE_METRE]
    NetArea = 0.070673092907964932 [SQUARE_METRE]
    NetVolume = 0.4242338130680437 [CUBIC_METRE]
  Qto_SlabBaseQuantities | quantities | on 2 objects (2 IFCSLAB)
    Depth = 6000. [MILLI METRE]
    GrossArea = 0.070673092907964946 [SQUARE_METRE]
    NetArea = 0.070673092907964946 [SQUARE_METRE]
    NetVolume = 0.42423381306804347 [CUBIC_METRE]
  Qto_SlabBaseQuantities | quantities | on 2 objects (2 IFCSLAB)
    Depth = 299.99999999999989 [MILLI METRE]
    GrossArea = 0.35999999999999999 [SQUARE_METRE]
    GrossVolume = 0.10799999999999996 [CUBIC_METRE]
    Length = 600. [MILLI METRE]
    NetArea = 0.35999999999999999 [SQUARE_METRE]
    NetVolume = 0.10799999999999997 [CUBIC_METRE]
    Perimeter = 2400. [MILLI METRE]
    Width = 600. [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 2 objects (2 IFCSLAB)
    Depth = 6000. [MILLI METRE]
    GrossArea = 0.070673092907964946 [SQUARE_METRE]
    NetArea = 0.070673092907964946 [SQUARE_METRE]
    NetVolume = 0.42423381306804292 [CUBIC_METRE]
  Qto_SlabBaseQuantities: 15 more contents on 17 objects not shown
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 3. (IFCCOUNTMEASURE)
    NumberOfTreads = 3. (IFCCOUNTMEASURE)
    Reference = "190mm max riser 250mm going" (IFCIDENTIFIER)
    RiserHeight = 180.00000000000827 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtInnerSide = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 4.4035433070835719 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 type object
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 0. (IFCCOUNTMEASURE)
    NumberOfTreads = 0. (IFCCOUNTMEASURE)
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIR)
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 3. (IFCCOUNTMEASURE)
    NumberOfTreads = 3. (IFCCOUNTMEASURE)
    Reference = "190mm max riser 250mm going" (IFCIDENTIFIER)
    RiserHeight = 180.00000000000827 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtInnerSide = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 4.4035433070835719 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 3. (IFCCOUNTMEASURE)
    NumberOfTreads = 3. (IFCCOUNTMEASURE)
    Reference = "50 mm Tread 13 mm Riser" (IFCIDENTIFIER)
    RiserHeight = 180.00000000000827 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtInnerSide = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 4.4035433070835719 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairFlightCommon | properties | on 1 type object
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 0. (IFCCOUNTMEASURE)
    NumberOfTreads = 0. (IFCCOUNTMEASURE)
  Pset_MemberCommon | properties | on 40 objects (40 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "SC15012" (IFCIDENTIFIER)
    Roll = -45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 3000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 40 objects (40 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "SC15012" (IFCIDENTIFIER)
    Roll = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 3000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 8 objects (8 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "SC15012" (IFCIDENTIFIER)
    Roll = -45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 4500. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 8 objects (8 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "SC15012" (IFCIDENTIFIER)
    Roll = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 4500. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 6 objects (6 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "88.9x5.0CHS" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 3000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Stringer - 50 mm Width" (IFCIDENTIFIER)
    Slope = 30.963756532074704 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 5 type objects
    LoadBearing = TRUE (IFCBOOLEAN)
  Qto_MemberBaseQuantities | quantities | on 13 objects (13 IFCMEMBER)
    CrossSectionArea = 0.00036237944995207193 [SQUARE_METRE]
    GrossSurfaceArea = 1.7162408970373451 [SQUARE_METRE]
    GrossVolume = 0.0010291576378638854 [CUBIC_METRE]
    Length = 3000. [MILLI METRE]
    NetSurfaceArea = 1.7162408970373453 [SQUARE_METRE]
    NetVolume = 0.0010291678906710943 [CUBIC_METRE]
    OuterSurfaceArea = 1.7155161381374409 [SQUARE_METRE]
  Qto_MemberBaseQuantities | quantities | on 9 objects (9 IFCMEMBER)
    CrossSectionArea = 0.00036237944995207193 [SQUARE_METRE]
    GrossSurfaceArea = 1.7162408970373451 [SQUARE_METRE]
    GrossVolume = 0.0010291576378638854 [CUBIC_METRE]
    Length = 3000. [MILLI METRE]
    NetSurfaceArea = 1.7162408970373453 [SQUARE_METRE]
    NetVolume = 0.0010291678906712344 [CUBIC_METRE]
    OuterSurfaceArea = 1.7155161381374409 [SQUARE_METRE]
  Qto_MemberBaseQuantities | quantities | on 6 objects (6 IFCMEMBER)
    CrossSectionArea = 0.00036237944995207193 [SQUARE_METRE]
    GrossSurfaceArea = 1.7162408970373451 [SQUARE_METRE]
    GrossVolume = 0.0010291576378638854 [CUBIC_METRE]
    Length = 3000. [MILLI METRE]
    NetSurfaceArea = 1.7162408970373453 [SQUARE_METRE]
    NetVolume = 0.0010291678906710797 [CUBIC_METRE]
    OuterSurfaceArea = 1.7155161381374409 [SQUARE_METRE]
  Qto_MemberBaseQuantities | quantities | on 6 objects (6 IFCMEMBER)
    CrossSectionArea = 0.00036237944995207193 [SQUARE_METRE]
    GrossSurfaceArea = 1.7162408970373451 [SQUARE_METRE]
    GrossVolume = 0.0010291576378638854 [CUBIC_METRE]
    Length = 3000. [MILLI METRE]
    NetSurfaceArea = 1.7162408970373453 [SQUARE_METRE]
    NetVolume = 0.0010291678906712328 [CUBIC_METRE]
    OuterSurfaceArea = 1.7155161381374409 [SQUARE_METRE]
  Qto_MemberBaseQuantities | quantities | on 5 objects (5 IFCMEMBER)
    CrossSectionArea = 0.00036237944995207193 [SQUARE_METRE]
    GrossSurfaceArea = 1.7162408970373451 [SQUARE_METRE]
    GrossVolume = 0.0010291576378638854 [CUBIC_METRE]
    Length = 3000. [MILLI METRE]
    NetSurfaceArea = 1.7162408970373453 [SQUARE_METRE]
    NetVolume = 0.0010291678906711001 [CUBIC_METRE]
    OuterSurfaceArea = 1.7155161381374409 [SQUARE_METRE]
  Qto_MemberBaseQuantities | quantities | on 5 objects (5 IFCMEMBER)
    CrossSectionArea = 0.00036237944995207193 [SQUARE_METRE]
    GrossSurfaceArea = 1.7162408970373451 [SQUARE_METRE]
    GrossVolume = 0.0010291576378638854 [CUBIC_METRE]
    Length = 3000. [MILLI METRE]
    NetSurfaceArea = 1.7162408970373453 [SQUARE_METRE]
    NetVolume = 0.0010291678906710821 [CUBIC_METRE]
    OuterSurfaceArea = 1.7155161381374409 [SQUARE_METRE]
  Qto_MemberBaseQuantities | quantities | on 5 objects (5 IFCMEMBER)
    CrossSectionArea = 0.00036237944995207193 [SQUARE_METRE]
    GrossSurfaceArea = 1.7162408970373451 [SQUARE_METRE]
    GrossVolume = 0.0010291576378638854 [CUBIC_METRE]
    Length = 3000. [MILLI METRE]
    NetSurfaceArea = 1.7162408970373453 [SQUARE_METRE]
    NetVolume = 0.0010291678906712415 [CUBIC_METRE]
    OuterSurfaceArea = 1.7155161381374409 [SQUARE_METRE]
  Qto_MemberBaseQuantities | quantities | on 4 objects (4 IFCMEMBER)
    CrossSectionArea = 0.00036237944995207193 [SQUARE_METRE]
    GrossSurfaceArea = 1.7162408970373451 [SQUARE_METRE]
    GrossVolume = 0.0010291576378638854 [CUBIC_METRE]
    Length = 3000. [MILLI METRE]
    NetSurfaceArea = 1.7162408970373453 [SQUARE_METRE]
    NetVolume = 0.0010291678906710782 [CUBIC_METRE]
    OuterSurfaceArea = 1.7155161381374409 [SQUARE_METRE]
  Qto_MemberBaseQuantities: 28 more contents on 51 objects not shown
  Qto_StairFlightBaseQuantities | quantities | on 1 object (1 IFCSTAIRFLIGHT)
    GrossVolume = 0.0060398999999960431 [CUBIC_METRE]
    Length = 900.00000000000011 [MILLI METRE]
    NetVolume = 0.13723994999990591 [CUBIC_METRE]
  Qto_ColumnBaseQuantities | quantities | on 12 objects (12 IFCCOLUMN)
    CrossSectionArea = 0.0039273604210249401 [SQUARE_METRE]
    GrossVolume = 0.01096911765592266 [CUBIC_METRE]
    Length = 2793. [MILLI METRE]
    NetVolume = 0.0046582194363728926 [CUBIC_METRE]
    OuterSurfaceArea = 1.1735345417314091 [SQUARE_METRE]
  Qto_ColumnBaseQuantities | quantities | on 4 objects (4 IFCCOLUMN)
    CrossSectionArea = 0.003229777738071404 [SQUARE_METRE]
    GrossVolume = 0.010012310988021354 [CUBIC_METRE]
    Length = 3100. [MILLI METRE]
    NetVolume = 0.010012613800922993 [CUBIC_METRE]
    OuterSurfaceArea = 2.8244730826250852 [SQUARE_METRE]
  Qto_ColumnBaseQuantities | quantities | on 4 objects (4 IFCCOLUMN)
    CrossSectionArea = 0.003229777738071404 [SQUARE_METRE]
    GrossVolume = 0.010012310988021354 [CUBIC_METRE]
    Length = 3100. [MILLI METRE]
    NetVolume = 0.010012613800922996 [CUBIC_METRE]
    OuterSurfaceArea = 2.8244730826250848 [SQUARE_METRE]
  Qto_ColumnBaseQuantities | quantities | on 3 objects (3 IFCCOLUMN)
    CrossSectionArea = 0.003229777738071404 [SQUARE_METRE]
    GrossVolume = 0.011501238525272271 [CUBIC_METRE]
    Length = 3561.0000000000005 [MILLI METRE]
    NetVolume = 0.011501586369382841 [CUBIC_METRE]
    OuterSurfaceArea = 3.2444995636219125 [SQUARE_METRE]
  Qto_ColumnBaseQuantities | quantities | on 3 objects (3 IFCCOLUMN)
    CrossSectionArea = 0.003229777738071404 [SQUARE_METRE]
    GrossVolume = 0.02325439971411411 [CUBIC_METRE]
    Length = 7200.0000000000009 [MILLI METRE]
    NetVolume = 0.023255103021498569 [CUBIC_METRE]
    OuterSurfaceArea = 6.5600665144840686 [SQUARE_METRE]
  Qto_ColumnBaseQuantities | quantities | on 3 objects (3 IFCCOLUMN)
    CrossSectionArea = 0.003229777738071404 [SQUARE_METRE]
    GrossVolume = 0.01175316118884184 [CUBIC_METRE]
    Length = 3639. [MILLI METRE]
    NetVolume = 0.011753516652115744 [CUBIC_METRE]
    OuterSurfaceArea = 3.3155669508621557 [SQUARE_METRE]
  Qto_ColumnBaseQuantities | quantities | on 1 object (1 IFCCOLUMN)
    CrossSectionArea = 0.20249999999999999 [SQUARE_METRE]
    GrossVolume = 0.60750000000000004 [CUBIC_METRE]
    Length = 3000. [MILLI METRE]
    NetVolume = 0.60749999999999982 [CUBIC_METRE]
    OuterSurfaceArea = 5.4000000000000004 [SQUARE_METRE]
  Pset_ColumnCommon | properties | on 17 objects (17 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "200UB25.4" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 12 objects (12 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HSS63.5X63.5X7.9" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "450 x 450mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 7 type objects
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_ReinforcementBarPitchOfColumn | properties | on 17 objects (17 IFCCOLUMN)
    Reference = "200UB25.4" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 12 objects (12 IFCCOLUMN)
    Reference = "HSS63.5X63.5X7.9" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN)
    Reference = "450 x 450mm" (IFCLABEL)
  Pset_BeamCommon | properties | on 54 objects (54 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Timber_50 x200" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 1500. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 52 objects (52 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Timber_50 x200" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 3000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 52 objects (52 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Timber_50 x150 _ContentGenerator" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 3000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 27 objects (27 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "356mm" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 6027. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 13 objects (13 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Timber_50 x150 _ContentGenerator" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 2973.7999999999824 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 12 objects (12 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "88.9x5.0CHS" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 3000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 11 objects (11 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "200UB25.4" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 45.000549477047585 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 4242.6000000000004 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 5 objects (5 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "200UB25.4" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 5867.1999999999998 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon: 18 more contents on 42 objects not shown
  Pset_ReinforcementBarPitchOfBeam | properties | on 106 objects (106 IFCBEAM)
    Reference = "Timber_50 x200" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 65 objects (65 IFCBEAM)
    Reference = "Timber_50 x150 _ContentGenerator" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 35 objects (35 IFCBEAM)
    Reference = "200UB25.4" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 27 objects (27 IFCBEAM)
    Reference = "356mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 16 objects (16 IFCBEAM)
    Reference = "30mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 12 objects (12 IFCBEAM)
    Reference = "88.9x5.0CHS" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 7 objects (7 IFCBEAM)
    Reference = "200PFC" (IFCLABEL)
  Qto_BeamBaseQuantities | quantities | on 9 objects (9 IFCBEAM)
    CrossSectionArea = 0.068350000000000508 [SQUARE_METRE]
    GrossSurfaceArea = 0.70350000000000035 [SQUARE_METRE]
    GrossVolume = 0.013670000000000149 [CUBIC_METRE]
    Length = 1500.0000000000011 [MILLI METRE]
    NetSurfaceArea = 0.70350000000000024 [SQUARE_METRE]
    NetVolume = 0.01367000000000013 [CUBIC_METRE]
    OuterSurfaceArea = 0.5667999999999993 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 7 objects (7 IFCBEAM)
    CrossSectionArea = 0.14334795602234909 [SQUARE_METRE]
    GrossSurfaceArea = 1.4534795602234809 [SQUARE_METRE]
    GrossVolume = 0.028669591204469914 [CUBIC_METRE]
    Length = 3000.0000000000014 [MILLI METRE]
    NetSurfaceArea = 1.4534795602234805 [SQUARE_METRE]
    NetVolume = 0.028669591204469894 [CUBIC_METRE]
    OuterSurfaceArea = 1.1667836481787828 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 7 objects (7 IFCBEAM)
    CrossSectionArea = 0.14334999999999926 [SQUARE_METRE]
    GrossSurfaceArea = 1.1617999999999875 [SQUARE_METRE]
    GrossVolume = 0.021502499999999983 [CUBIC_METRE]
    Length = 3000.0000000000023 [MILLI METRE]
    NetSurfaceArea = 1.1617999999999875 [SQUARE_METRE]
    NetVolume = 0.02150249999999982 [CUBIC_METRE]
    OuterSurfaceArea = 0.875099999999989 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 7 objects (7 IFCBEAM)
    CrossSectionArea = 0.14334999999999926 [SQUARE_METRE]
    GrossSurfaceArea = 1.1617999999999875 [SQUARE_METRE]
    GrossVolume = 0.021502499999999983 [CUBIC_METRE]
    Length = 2999.9999999999982 [MILLI METRE]
    NetSurfaceArea = 1.1617999999999875 [SQUARE_METRE]
    NetVolume = 0.02150249999999982 [CUBIC_METRE]
    OuterSurfaceArea = 0.875099999999989 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 6 objects (6 IFCBEAM)
    CrossSectionArea = 0.0062063367019324954 [SQUARE_METRE]
    GrossSurfaceArea = 0.80603628035066166 [SQUARE_METRE]
    GrossVolume = 0.017635926372211383 [CUBIC_METRE]
    Length = 3000. [MILLI METRE]
    NetSurfaceArea = 1.5006074638256761 [SQUARE_METRE]
    NetVolume = 0.0037430019355998976 [CUBIC_METRE]
    OuterSurfaceArea = 0.79362360694679668 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 6 objects (6 IFCBEAM)
    CrossSectionArea = 0.14335000000000128 [SQUARE_METRE]
    GrossSurfaceArea = 1.4535000000000029 [SQUARE_METRE]
    GrossVolume = 0.028670000000000351 [CUBIC_METRE]
    Length = 2999.9999999999959 [MILLI METRE]
    NetSurfaceArea = 1.4535000000000027 [SQUARE_METRE]
    NetVolume = 0.028670000000000334 [CUBIC_METRE]
    OuterSurfaceArea = 1.1668000000000003 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 6 objects (6 IFCBEAM)
    CrossSectionArea = 0.54243000000000063 [SQUARE_METRE]
    GrossSurfaceArea = 1.5742200000010962 [SQUARE_METRE]
    GrossVolume = 0.021697200000048558 [CUBIC_METRE]
    Length = 6027. [MILLI METRE]
    NetSurfaceArea = 3.7687957120207334 [SQUARE_METRE]
    NetVolume = 0.045937548800130852 [CUBIC_METRE]
    OuterSurfaceArea = 0.48936000000109492 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 6 objects (6 IFCBEAM)
    CrossSectionArea = 0.14334999999999926 [SQUARE_METRE]
    GrossSurfaceArea = 1.1617999999999875 [SQUARE_METRE]
    GrossVolume = 0.021502499999999983 [CUBIC_METRE]
    Length = 3000.0000000000023 [MILLI METRE]
    NetSurfaceArea = 1.1617999999999875 [SQUARE_METRE]
    NetVolume = 0.021502499999999976 [CUBIC_METRE]
    OuterSurfaceArea = 0.875099999999989 [SQUARE_METRE]
  Qto_BeamBaseQuantities: 125 more contents on 214 objects not shown
  Pset_FootingCommon | properties | on 4 objects (4 IFCFOOTING)
    Reference = "Bearing Footing - 900 x 300" (IFCIDENTIFIER)
  Pset_ReinforcementBarCountOfIndependentFooting | properties | on 4 objects (4 IFCFOOTING)
    Reference = "Bearing Footing - 900 x 300" (IFCLABEL)
  Pset_ReinforcementBarPitchOfContinuousFooting | properties | on 4 objects (4 IFCFOOTING)
    Reference = "Bearing Footing - 900 x 300" (IFCLABEL)
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    CrossSectionArea = 8.9442899999999383 [SQUARE_METRE]
    GrossSurfaceArea = 24.391439999999825 [SQUARE_METRE]
    GrossVolume = 2.6832869999999813 [CUBIC_METRE]
    Height = 899.99999999999238 [MILLI METRE]
    Length = 9628.0999999999094 [MILLI METRE]
    NetVolume = 2.6832869999999795 [CUBIC_METRE]
    OuterSurfaceArea = 6.5028599999999477 [SQUARE_METRE]
    Width = 900.00000000000011 [MILLI METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    CrossSectionArea = 18.518370252211138 [SQUARE_METRE]
    GrossSurfaceArea = 49.937069204206622 [SQUARE_METRE]
    GrossVolume = 5.5555110756633415 [CUBIC_METRE]
    Length = 21443.864017669654 [MILLI METRE]
    NetVolume = 5.5555110756633415 [CUBIC_METRE]
    OuterSurfaceArea = 12.900328699784346 [SQUARE_METRE]
    Width = 900.00000000000011 [MILLI METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    CrossSectionArea = 6.8407181831396562 [SQUARE_METRE]
    GrossSurfaceArea = 19.164791471531238 [SQUARE_METRE]
    GrossVolume = 2.0522154549418969 [CUBIC_METRE]
    Length = 8051.5703564887417 [MILLI METRE]
    NetVolume = 2.0522154549418965 [CUBIC_METRE]
    OuterSurfaceArea = 5.483355105251924 [SQUARE_METRE]
    Width = 900.00000000000011 [MILLI METRE]
  Qto_FootingBaseQuantities | quantities | on 1 object (1 IFCFOOTING)
    CrossSectionArea = 14.242699778781343 [SQUARE_METRE]
    GrossSurfaceArea = 38.918157591552657 [SQUARE_METRE]
    GrossVolume = 4.2728099336344032 [CUBIC_METRE]
    Length = 16229.092850365094 [MILLI METRE]
    NetVolume = 4.2728099336344059 [CUBIC_METRE]
    OuterSurfaceArea = 10.432758033989966 [SQUARE_METRE]
    Width = 900.00000000000011 [MILLI METRE]
  Pset_ElementComponentCommon | properties | on 334 objects (334 IFCREINFORCINGBAR)
    Reference = "Structural Rebar 1" (IFCIDENTIFIER)
  Pset_ElementComponentCommon | properties | on 12 objects (12 IFCREINFORCINGBAR)
    Reference = "Structural Rebar 12mm" (IFCIDENTIFIER)
  Pset_ReinforcingBarCommon | properties | on 82 objects (82 IFCREINFORCINGBAR)
    BarLength = 4650. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "Structural Rebar 1" (IFCIDENTIFIER)
  Pset_ReinforcingBarCommon | properties | on 72 objects (72 IFCREINFORCINGBAR)
    BarLength = 1440. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "Structural Rebar 1" (IFCIDENTIFIER)
  Pset_ReinforcingBarCommon | properties | on 12 objects (12 IFCREINFORCINGBAR)
    BarLength = 1300.3154676095169 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "Structural Rebar 12mm" (IFCIDENTIFIER)
  Pset_ReinforcingBarCommon | properties | on 6 objects (6 IFCREINFORCINGBAR)
    BarLength = 20676.721492004399 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "Structural Rebar 1" (IFCIDENTIFIER)
  Pset_ReinforcingBarCommon | properties | on 6 objects (6 IFCREINFORCINGBAR)
    BarLength = 1150. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "Structural Rebar 1" (IFCIDENTIFIER)
  Pset_ReinforcingBarCommon | properties | on 6 objects (6 IFCREINFORCINGBAR)
    BarLength = 1006.2300798097085 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "Structural Rebar 1" (IFCIDENTIFIER)
  Pset_ReinforcingBarCommon | properties | on 6 objects (6 IFCREINFORCINGBAR)
    BarLength = 1006.2300798097956 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "Structural Rebar 1" (IFCIDENTIFIER)
  Pset_ReinforcingBarCommon | properties | on 6 objects (6 IFCREINFORCINGBAR)
    BarLength = 1321.5878642412399 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "Structural Rebar 1" (IFCIDENTIFIER)
  Pset_ReinforcingBarCommon: 97 more contents on 150 objects not shown
  Pset_ElementAssemblyCommon | properties | on 16 objects (16 IFCELEMENTASSEMBLY)
    Reference = "Structural Framing System" (IFCIDENTIFIER)